Main Control Computer Communication Protocol

# Received message

## Command messages

CMD\_SEND\_STORED\_MEASUREMENTS

CAN ID:

Class: 0x0C

Device: 0x01

Type: 0x00 (CAN\_MESSAGETYPE\_COMMAND)

DLC: 1

Data:

| Byte offset | Format | Name | Code |
| --- | --- | --- | --- |
| 0 | U8 | CMD\_SEND\_MEAS | 0x5C |

# Sent message

## Measurement messages

STORED\_MEASUREMENTS

CAN ID:

Class: 0x0C

Device: 0x01

Type: 0x03 (CAN\_MESSAGETYPE\_COMMAND)

DLC: 5-8

Data:

| Byte offset | Format | Name | Code |
| --- | --- | --- | --- |
| 0 | U8 | HEADER | value |
| 1 | F32 | MEAS\_DATA | value |